Name :Immediate output

Symbol:OUT_IMMEDIATELY

Illustrate:

        You can use the Output Now function to immediately output a specified value to a Q-zone address, but only one BOOL address

Image:

Parameter:

Parameter | Statement | Type | Description
--- | --- | --- | ---
ADDR | Input | UDINT |
    Q output address, for example, %QBm
OFFSET | Input | USINT |
    The Q address is offset, for example, %QXm.n, and the input value should be less than 8
VALUE | Input | BOOL |
    The value is output immediately, 1 is output if TRUE, and 0 is output if FALSE
OUT | Output | BOOL |
    The function returns a value, 1 for success and 0 for failure

Example:

LD:

ST:

OUT_IMMEDIATELY(ADDR := 1, OFFSET := 2, VALUE := TRUE);

Interpretation:

       ADDR为1，表示Q区输出地址为%QB1，OFFSET为2，表示Q区地址偏移为2，输出地址为%QX1.2，VALUE为TRUE表示输出值为1。