Name :PLC downtime

Symbol :SYS_STOP

Illustrate:

        Stop the application of the PLC.

Image:

Parameter:

Parameter | Statement | Type | Description
--- | --- | --- | ---
EXECUTE | Input | BOOL |
    Ascending edge execution
DONE | Output | BOOL |
    finish

Example:

LD:

ST:

SYS_STOP_inst1(EXECUTE := bExecute, DONE =>bDONE);

Interpretation:

         When the signal status of the "bExecute" operand changes from "0" to "1", the command is executed, the application is stopped, and the signal status of the output of "DONE" is "1".